Full-Body Harness Annual Inspection

|  |  |  |
| --- | --- | --- |
| Harness Mfr./Model/Name | | |
| Serial Number | Lot Number | |
| Date of Manufacture Click to enter date | Date of Purchase Click to enter date | |
| Inspected By (Competent Person) | | Date Inspected Click to enter date |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Components** | | **Pass** | **Fail** | **Comments** |
| **Hardware** | | | | |
| 1 | Inspect D-rings, buckles, keepers and back pads. Inspect for damage, distortion, sharp edges, burrs, cracks, and corrosion |  |  |  |
| 2 | Other: |  |  |  |
| **Webbing** | | **Pass** | **Fail** |  |
| 3 | Inspect for cuts, burns, tears, abrasions, frays, excessive soiling and discoloration |  |  |  |
| 4 | Other: |  |  |  |
| **Stitching** | | **Pass** | **Fail** |  |
| 5 | Inspect for pulled or cut stitches |  |  |  |
| 6 | Other: |  |  |  |
| **Labels** | | **Pass** | **Fail** |  |
| 7 | Inspect, making certain all labels are securely held in place and are legible |  |  |  |
| **Other** | | **Pass** | **Fail** |  |
| 8 |  |  |  |  |
| **Overall Assessment** | | **Pass** | **Fail** |  |
|  |  |  |
| Comments: Click to enter text | | | | |

**If harness fails, it must be tagged and taken out of service.**